Health & Safety Module - Machinery
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	Select a machine that you are familiar with and identify the ways in which the controls have been designed to prevent danger

	Conventional lathe – guarding is strong enough to withstand vibration and wear caused by normal functioning of machine and is of sufficient strength to protect operator.  Emergency stop button easily accessible

	What are the hazards when using this machine?

	Entanglement and contact with cutters or rotating components when:

Loading or unloading components, removing swarf, measuring, adjusting coolant flow.
Eye injuries from ejected particles

Noise causing hearing damage

Cuts from swarf removal

	How are they controlled?

	Through training, use of guarding & eye protection. No loose clothing to be worn and hair to be tied back or hat worn to prevent entanglement. Hearing protection to be worn when required. Swarf hook or brush to be used to prevent cuts to hands.

	What harmful substances could you be exposed to when using this machine & how is this hazard controlled?

	Cutting oils in use can cause skin irritation. Gloves and barrier creams available and in use. Data sheet available on substances used listing hazards and controls to be applied.

	Are manual handling hazards present in the process?

	Trolley available to move heavy bins of components. Hoist in use to load heavy components and all operators trained to use hoist safely.

	If you have concerns regarding the safety of a piece of equipment, who should you contact within your company?


	Mr A. Mentor (Supervisor)

	Our training officer will want to check your knowledge of the above 
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